# Charging Infrastructure

Charge with confidence — a growing network of stations plus home and depot charging support.

Compatibility

## Connector Types Available

🔌
Type 2 (AC)
Up to 22 kW

Standard AC charging for home, office and overnight depot charging.

⚡
CCS2 (DC)
Up to 120 kW

DC fast charging for quick top-ups on the go at our highway stations.

🔋
GB/T (DC)
Up to 60 kW

Widely available DC standard, compatible with our van line-up.

## How Long Does Charging Take?

Typical times for a Green Automobiles EV van (42 kWh battery).

DC Fast Charge (20% → 80%)~ 45–60 min
AC Home Charge (0% → 100%)~ 6–8 hours
Standard Socket (trickle)~ 12+ hours
Our Network

## Charging Stations

View on map →
Kalanki Hub Live
Kalanki Chowk, Kathmandu
Type
DC Fast
Ports
4
Prithvi Chowk Live
Pokhara
Type
DC Fast
Ports
2
Traffic Chowk Live
Butwal
Type
AC + DC
Ports
3
Narayangarh Live
Bharatpur, Chitwan
Type
DC Fast
Ports
2
Main Road Station Coming soon
Biratnagar
Type
AC
Ports
2
Surkhet Road Live
Nepalgunj
Type
DC Fast
Ports
2